**Advanced Pitch Angle Control based on Genetıc Algorıthm and Particle Swarm Optımızatıon for Variable-Speed on Fast systems**

***Goksu GOREL1,\*, Mahdi OSMAN ABDI2***

*1Institute of Science, Faculty of Engineering, Electric and Electronic department, Cankiri Karatekin university, Cankiri, Turkey*

*2* *Institute of Science, Faculty of Engineering, Electric and Electronic department, Cankiri Karatekin university, Cankiri, Turkey*

|  |
| --- |
|  **Abstract**This study looks into how wind turbines' rotor speed quality is improving as their mechanical loads are getting lighter. The wind turbine's rotor speed is kept constant by changing the blade angle to the nominal wind speed [1]. Different outcomes can be retrieved using control approaches (such PI, genetic algorithms, and particle swarm optimization) [2, 3, 4]. Additionally, we were able to lower the mechanical stresses on the turbine using the control methods thanks to the individual control of the blade tilt angle. Matlab/Simulink was used to model the wind turbine. |
| Keywords: Individual pitch control, Wind turbine, Fast system, Genetic algorithm, Particle swarm optimization  |

**References**

1. Bossanyi, E. A. (2005). Further load reductions with individual pitch control.  *Wind Energy: An International Journal for Progress and Applications in Wind Power Conversion Technology*, 8(4), 481-485.
2. Luy, M., Civelek, Z., & Cam, E. (2017). Individual pitch control on wind turbines with permanent magnet synchronous generator for reduction of mechanical load and stability of output power.  *Pamukkale University Journal of Engineering Sciences*, 23(5):504-511
3. Jayachitra, A., & Vinodha, R. (2014). Genetic Algorithm Based PID Controller Tuning Approach for Continuous Stirred Tank Reactor.  *Advances in Artificial Intelligence,* 16877470.
4. GirirajKumar, S. M., Jayaraj, D., & Kishan, A. R. (2010). PSO based tuning of a PID controller for a high performance drilling machine. *International Journal of Computer Applications*, 1(19), 12-18.