**Electrocoating of Polyaniline and Polypyrrole from Deep Eutectic Solution**

***Asuman UNAL1[C:\Users\Abdullah\AppData\Local\Microsoft\Windows\INetCache\Content.Word\ORCID-iD_icon-16x16.gif](https://orcid.org/0000-xxxx-xxxx-xxxx)***

*1Department of Chemistry, Faculty of Science, Cankiri Karatekin University, Cankiri, 18200, Turkey*

|  |
| --- |
| **Abstract**  The high conductivity, chemical stability and simple synthesis of polyaniline and polypyrrole have given these polymers a wide range of applications in energy storage devices, chemical sensors and biosensors [1,2]. Polyaniline and polypyrrole, which are the conducting polymers, have been produced by electrochemical and chemical methods in aqueous and non-aqueous media [3,4]. However, the synthesis of these polymers in an aqueous medium may result in loss of electroactive sites of the final polymer films [5]. On the other hand, using a non-aqueous medium during electrochemical synthesis can improve not only electrochemical properties but also physical properties of the final polymer films [6]. Therefore, this study focused on the synthesis of polyaniline and polypyrrole from deep eutectic solvents under optimal conditions, and the findings show that the use of a non-aqueous medium provides more homogeneous and better electroactive polymer film production than aqueous media.  **Keywords:** *Conducting polymers; Polynailine; Polypyrrole; Deep eutectic solvents* |
|  |

**References**

[1] A.A. Syed, M.K. Dinesan, Review: Polyaniline-A novel polymeric material, Talanta. (1991). doi:10.1016/0039-9140(91)80261-W.

[2] A.A. Ganash, Electrochemical synthesis and corrosion behaviour of polypyrrole and polypyrrole/carbon nanotube nanocomposite films, J. Compos. Mater. (2014). doi:10.1177/0021998313495904.

[3] A.F. Diaz, J.I. Castillo, A polymer electrode with variable conductivity: Polypyrrole, J. Chem. Soc. - Ser. Chem. Commun. (1980). doi:10.1039/C39800000397.

[4] A. Malinauskas, Chemical deposition of conducting polymers, Polymer (Guildf). (2001). doi:10.1016/S0032-3861(00)00800-4.

[5] P. Gajendran, R. Saraswathi, Polyaniline-carbon nanotube composites, in: Pure Appl. Chem., 2008. doi:10.1351/pac200880112377.

[6] P.M.V. Fernandes, J.M. Campiña, C.M. Pereira, F. Silva, Electrosynthesis of polyaniline from choline-based deep eutectic solvents: Morphology, stability and electrochromism, J. Electrochem. Soc. (2012). doi:10.1149/2.059209jes.